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SPECIFICATION
Hippo-M MAX Connector
10mm PCB 2 Pins for COB/SMD
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Basic Info
	Product Series
	Hippo-M MAX
	
	

	[bookmark: OLE_LINK1]Item NO.
	[bookmark: OLE_LINK2]MX/2045-X10C-2P
	MX/2045-B10C-2P
	MX10BXB-L2C

	Connection Type
	Strip to Wire
	Strip to Strip Joint
	Corner Strip to Strip Bridge

	With Wire or NOT
	No wire
	No wire
	with wire (20AWG/0.52mm²)


Physical Data
	Item NO.
	MX/2045-X10C-2P
	MX/2045-B10C-2P
	MX10BXB-L2C

	Shape
	I shape, straight connection
	I shape, straight connection
	L shape, Corner connection

	Size
	19*12.6*6.2
	19.8*12.6*6.2 
	36.6*36.6*6.2

	Pin Quantity
	2
	2
	2

	Notch Width
	5.0mm
	5.0mm
	5.0mm


Size detail, pls refer to below Dimensional Diagram
Material Data
	Housing Color
	Transparent

	Material
	Polycarbonate(PC), Phosphor bronze

	Surface Treatment
	Nickel plating

	Housing Deform Temperature
	80℃


Electrical Data
	Item NO.
	MX/2045-X10C-2P
	MX/2045-B10C-2P
	MX10BXB-L2C

	Voltage
	DC3~48V
	DC3~48V
	DC3~48V



Current & Temperature 
	Item NO.
	Max Current
	PCB Copper Thickness Required
	Temperature Raise (ΔT)
	Max LED Strip Temperature T(strip)

	MX/2045-X10C-2P
	4A
	2 OZ
	10℃
	65℃

	
	5.0A
	3 OZ
	10℃
	65℃

	MX/2045-B10C-2P
	3.0A
	2 OZ
	10℃
	65℃

	
	4.0A
	3 OZ
	10℃
	65℃

	MX10BXB-L2C
	4A
	2 OZ
	10℃
	65℃

	
	5.0A
	3 OZ
	10℃
	65℃


Note: Test with @TA=30℃ Wire Gauge=20AWG
Remark
1. ΔT = Inner Temperature Raise for reference; 
2. T(strip) = temperature of working led strip
3. In actual application, make sure T(strip) doesn't exceed the highest temperature listed above
( For example T(strip)<=60℃) otherwise lower the pcb current or apply extra cooling for long term working
Workable LED Strip
	Type
	COB/SMD

	Size（WxH）
	10x3.9 mm
	
	
	

	Light Color
	MONO
	
	
	

	IP Rating
	IP20 / IP65 silicon
	
	
	

	PCB Thickness
	0.25 ~0.35 mm
	
	
	

	LED Density/ Meter
	No Limited to COB，if SMD , it depends on SMD size


Workable Wire Data
	AItem NO.
	MX/2045-X10C-2P
	
	
	

	Wire Gauge
	Best fit 18AWG/0.78mm² (PVC) & 18AWG/0.78mm² (Teflon) ; 20AWG/0.52mm² (PVC)

	Outer Diameter
	MONO OD＜2.1mm
	
	


Working Environment
	Environment TEMP.
	-10 ~ 45℃

	Environment
	Indoor


Dimensional Diagram
	Item NO.:
	MX/2045-X10C-2P
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	Item NO.:
	MX/2045-B10C-2P
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	Item NO.:
	MX10BXB-L2C
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Tolerance（mm）
	Size Range
	Tolerance
	
	
	
	
	

	≤3
	±0.10
	
	
	
	
	

	＞3≤10
	±0.15
	
	
	
	
	

	＞10≤20
	±0.20
	
	
	
	
	

	＞20
	±0.25
	
	
	
	
	


If the diagram has marked the tolerance data, use it as a standard; If not , take the tolerance table as standard.


[bookmark: _GoBack]
image4.jpeg
6. 20

12. 60

12. 60

o)
S
o
=

6. 50

086l

NR "Al





image5.png
19. 00

12. 60

19. 00

12. 60
10. 05

6. 50

36.60

36.60




image2.jpeg




image3.png
19. 00

6. 20

12. 60

12. 60
10. 05

3.7

6. 50

19. 00

6. 20





image1.png
onlumi




